Welding Exam

Rubric



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **Poor****5 pts**  | **Fair****10 pts**  | **Good****15 pts**  | **Excellent****20 pts**  |
| **Slag on weld**  | Poor Weld not cleaned  | Fair Little removed  | Good Some remaining  | Excellent No Slag  |
| **Bead Width**  | Poor Varies within 3/16"  | Fair Varies within 1/8"  | Good Consistent and within 1/16"  | Excellent Consistent and within 1/32"  |
| **Bead Height**  | Poor Varies within 1/8  | Fair Varies within 1/16"  | Good Consistent and within 1/32"  | Excellent Consistent and within 1/64"  |
| **Weldment**  | Poor One of the four criteria met.  | Fair Two of the four criteria met.  | Good Three of the four criteria met.  | Excellent Weld starts on edge and finishes on edge. Welds are straight. Welds are touching. Two four inch welds per rod.  |
| **Appearance**  | Poor Uneven  | Fair 3 - 4 sections varied ripples  | Good 2 sections or less and even within sections  | Excellent Even ripples and smooth  |